cwi`k©b wUgbs -16 (‡lvj) KZ…©K gvV ch©v‡q Dbœqb Kg©Kv‡Ûi Dci cwi`k©b cÖwZ‡e`b

wUg AvnŸvqK I m`m¨M‡Yi bvg t (1) Rbve †gvt bvCg DwÏb wgqv, cÖKí cwiPvjK, AviwWAviAvBwWwc I AvnŸvqK, cwi`k©b wUg-16|

(2) Rbve †gvt bvwki DwÏb, wbe©vnx cÖ‡KŠkjx, AviwWAviAvBwWwc, GjwRBwW ,m`i `ßi, XvKv|

(3) জনাব মোহাম্মদ আহসান আলী, সিনিয়র সহকারী প্রকৌশলী, (ইউজিআইআইপি-৩)

cÖwZ‡e`b gvmt b‡f¤^i/2021

| µwgKbs | cwi`k©‡bi ZvwiL | ‡Rjv I Dc‡Rjv | cwi`k©bK…Z ¯‹x‡gi bvg | cÖK‡íi bvg | cwi`k©bK…Z ¯‹xg mg~‡ni cwijwÿZ ÎæwU/ mgm¨v mg~‡ni eY©bv (cÖ‡hvR¨ ‡ÿ‡Î my®úó †¯úwmwd‡Kkb Abyhvqx; †hgb (†Lvqvi mvBR /WBM Gi Thickness/ BZ¨vvw`) | | | ÎwU ms‡kvab/ mgm¨v mg~n mgvav‡bi Rb¨ mycvwikgvjv Ges M„nxZ e¨e¯’vvw` |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Item | Design Speci- fication | Field Observation |
| 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 |
| 01 | 15/11/  2021 | ivRkvnx, Zv‡bvi | Kv‡Ri bvg : Minor Maintenance of 30.90 Long RCC Girder Bridge on kashim Bazar Baya road at ch 5595.00m | SupRB | -Rail post  -Rail bar  -Approch protection  -Guide post  -cleaning | As per design and Specification | -Rail post, Rail bar I Guide post h\_vh\_fv‡e iO Kiv nq bvB|  -eªxR wbg©vY mvBU cwi®‹vi Kiv nq bvB| | * Rail post, Rail bar I Guide post mg~n h\_vh\_fv‡e iO Ki‡Z n‡e| * eªxR G‡cÖvP I wbg©vY¯’j cwi®‹vi Ki‡Z n‡e| |
| 02 | 15/11/2021 | ivRkvnx, Zv‡bvi | -Boundary wall Including gate of Primary School a) AKCHA, b) CHAPRA, c) Chinas. Ho d) DEBIpur GPS  Package No e- tender/ PEDP-4/Raj/Tan/2019-20/W14.0708 | PEDP-4 | column  Grade Beam  Brick work | As per Specification | -Column, Grade Beam and brick work completed  -Plaster ongoing | * Plaster Kv‡R curing h\_vh\_f‡e Ki‡Z n‡e| |
| 03 | 16/11/  2021 | ivRkvnx, Zv‡bvi | Periodic Maintenance of Kashim Bazar Baya Road Ch. 00-7850.00m | GOBM | -HBP  -BC  -Traffic  Sign | As per Specification | -iv¯Ívq unspecified traffic sign ¯’vcb Kiv n‡q‡Q| | * unspecified traffic sign mg~n Acmvib K‡i Design I Manual Abyhvqx mwVK traffic sign ¯’vc‡bi Rb¨ wb‡`©kbv cÖ`vb Kiv n‡q‡Q| |
| 04 | 16/11/  2021 | ivRkvnx, Zv‡bvi | Tanore –chowbaria road at ch. 2500-12640 m | RCIP | WMM  BC | WBM-100.00  BC-40m | **Ch. 2800m**  -WMM – 100.00m  -BC-42.00m  **Ch5730m**  -WMM – 95.00m  -BC-50.00m  - iv¯Ívi Shoulder G Negative Slope we`¨gvb| | * Nagative Shoulder h\_vh\_fv‡e wVK Ki‡Z n‡e| * Shoulder G wWRvBb I †¯úwmwd‡Kkb †gvZv‡eK gvwUi KvR Ki‡Z n‡e| |
| 05 | 17/11/  2021 | ivRkvnx, Zv‡bvi | Improvement of Talondo to Keshor hat (from hat shail) Road (Tanore part) at ch. 00-5440m | RCIP | WMM  Prime coat  BC | WMM- 75.00mm (Existing)  WMM-150.00mm (Widening) | **Ch. 1000m**  C/L wmm=76.00mm  L/S, wmm-150.00mm (widening)  **Ch. 1700m**  C/L wmm=76.00mm  R/S, wmm-155.00mm (widening)  -Prime coat completed  -ev¯ÍevwqZ Prime Coat Gi gvb fv‡jv, Z‡e wKQz wKQz RvqMvq Prime Coat bó n‡q †M‡Q| | * `ªæZ Carpeting Gi KvR m¤úbœ Ki‡Z n‡e| * Carpeting Gi c~‡e© bó Prime coat Specification ‡gvZv‡eK ms‡kvab Ki‡Z n‡e| * iv¯Ívi Shoulder I Slope G h\_vh\_fv‡e gvwUi KvR m¤úbœ Ki‡Z n‡e| |
| 06 | 18/11/  2021 | PuvcvBbeveMÄ | Construction of chapai Nawabganj diabetic hospital of 50 nos bed under sader upazila  Package No: C.Nawabgonj/DIABETIC/  C-1 | Construction of Diabetic Hospital (TS) | Building works | As per Specification | -RCC work completed  -Brick work 60% completed | * wbg©vb KvR PjvKvwjb mg‡q wbivcËv equipment’s e¨envi wbwðZ Ki‡Z n‡e| |

|  |  |  |
| --- | --- | --- |
| (‡gvnv¤§` Avnmvb Avjx)  wmwbqi mnKvix cÖ‡KŠkjx  BDwRc m`i `ßi| | (‡gvnvt bvwki DwÏb)  wbe©vnx cÖ‡KŠkjx  AviwWAviAvBwWwc| | (†gvt bvCg DwÏb wgqv)  cÖKí cwiPvjK  AviwWAviAvBwWwc  I  AvnŸvqK, cwi`k©b wUg-16| |